|  |
| --- |
| **Infrared thermal imaging core** |
| **Model#** | **FO-A317-V01** | **FO-H617-V04** | **FO-H612-V01** | **FO-H1212-V01** |
| **Sensor Performance** |
| Sensor type | VOx Uncooled FPA |
| Resolution | 384×288 | 640×512 | 640×512 | 1280×1024 |
| Pixel pitch | **17μm** | **12μm** |
| Frame Rate | 50Hz | 50Hz | 25Hz | 50Hz |
| Response wavelength | 8～14μm |
| NETD | ≤45mK@25℃ |
| **Image Adjustment** |
| Brightness and contrast | Manual/Auto |
| Polarity | Black hot/White hot |
| Pseudo-color | Multiple pseudo colors available |
| Reticle | Display/blank/move |
| Electronic zoom | 2x ,4x , 8x | 1-16x Stepless zoom |
| Image processing | Non-uniformity correction |
| Digital filter noise reduction |
| Digital detail enhancement |
| Image mirroring | Left/right;up/down;diagonal |
| **Software function** |
| Start-up interface | Gray and neutral screen without any words(customizable) |
| Boot time | ≤15S |
| Program upgrade | support serial port upgrade |
| **Lens control** |
| Lens type | Single FOV/dual FOV/continuous zoom |
| One-click focus | Support |
| Motorized focus | Continuous adjustment/fine adjustment |
| Electric autofocus &zoom | Continuous adjustment/fine adjustment |
| **Power supply** |
| Typical supply voltage | 12V DC |
| Power supply protection | Overvoltage, undervoltage, reverse connection |
| Typical power consumption | ＜1.8W | ＜2.2W | ＜2.2W@25℃ | ＜4.4W@25℃ |
| **Interface** |
| Analog Video output | 1 way PAL /NTSC | / |
| Digital Video output | LVDS/BT.656/BT.1120/SDI | SDI |
| Serial communication | RS232/RS485（Baud rate：115200（N,8,1）） |
| PELCO protocol |  |
| **Physical characteristics** |
| Weight (w/t lens) | ≤80g | ≤60g | ≤150g |
| Dimension (w/t lens) | 40mm×40mmx34mm | 34mmx34mmx34mm | 55mm×55mmx37mm |
| **Environmental adaptability** |
| Working temperature | -40℃～+60℃ |
| Working humidity | 0%～90%RH |
| Storage temperature | -45℃～+70℃ |
| Storage humidity | 0%～95%RH |
| Impulse Test | GJB150-18 Experiment 7 100g/6ms |
| Vibration Test | GJB150-16 2.3.1.1 |